LC_ALL=C \
PATH=/bin \
HOME=/tmp/lib/domain--1-guest \
USER=test \
LOGNAME=test \
XDG_DATA_HOME=/tmp/lib/domain--1-guest/.local/share \
XDG_CACHE_HOME=/tmp/lib/domain--1-guest/.cache \
XDG_CONFIG_HOME=/tmp/lib/domain--1-guest/.config \
QEMU_AUDIO_DRV=none \
/usr/bin/qemu-system-riscv64 \
-name guest=guest,debug-threads=on \
-S \
-object secret,id=masterKey0,format=raw,\
file=/tmp/lib/domain--1-guest/master-key.aes \
-machine virt,accel=tcg,usb=off,dump-guest-core=off \
-m 4096 \
-overcommit mem-lock=off \
-smp 4,sockets=4,cores=1,threads=1 \
-uuid 1ccfd97d-5eb4-478a-bbe6-88d254c16db7 \
-display none \
-no-user-config \
-nodefaults \
-chardev socket,id=charmonitor,fd=1729,server,nowait \
-mon chardev=charmonitor,id=monitor,mode=control \
-rtc base=utc \
-no-shutdown \
-boot strict=on \
-device pcie-root-port,port=0x8,chassis=1,id=pci.1,bus=pcie.0,multifunction=on,\
addr=0x1 \
-device pcie-root-port,port=0x9,chassis=2,id=pci.2,bus=pcie.0,addr=0x1.0x1 \
-device pcie-root-port,port=0xa,chassis=3,id=pci.3,bus=pcie.0,addr=0x1.0x2 \
-device pcie-root-port,port=0xb,chassis=4,id=pci.4,bus=pcie.0,addr=0x1.0x3 \
-device pcie-root-port,port=0xc,chassis=5,id=pci.5,bus=pcie.0,addr=0x1.0x4 \
-device pcie-root-port,port=0xd,chassis=6,id=pci.6,bus=pcie.0,addr=0x1.0x5 \
-device pcie-root-port,port=0xe,chassis=7,id=pci.7,bus=pcie.0,addr=0x1.0x6 \
-device qemu-xhci,p2=15,p3=15,id=usb,bus=pci.2,addr=0x0 \
-device virtio-serial-pci,id=virtio-serial0,bus=pci.3,addr=0x0 \
-drive file=/var/lib/libvirt/images/guest.qcow2,format=qcow2,if=none,\
id=drive-virtio-disk0 \
-device virtio-blk-pci,scsi=off,bus=pci.4,addr=0x0,drive=drive-virtio-disk0,\
id=virtio-disk0,bootindex=1 \
-netdev user,id=hostnet0 \
-device virtio-net-pci,netdev=hostnet0,id=net0,mac=52:54:00:09:a4:37,bus=pci.1,\
addr=0x0 \
-chardev pty,id=charserial0 \
-serial chardev:charserial0 \
-chardev socket,id=charchannel0,fd=1729,server,nowait \
-device virtserialport,bus=virtio-serial0.0,nr=1,chardev=charchannel0,\
id=channel0,name=org.qemu.guest_agent.0 \
-device virtio-balloon-pci,id=balloon0,bus=pci.5,addr=0x0 \
-object rng-random,id=objrng0,filename=/dev/urandom \
-device virtio-rng-pci,rng=objrng0,id=rng0,bus=pci.6,addr=0x0 \
-sandbox on,obsolete=deny,elevateprivileges=deny,spawn=deny,\
resourcecontrol=deny \
-msg timestamp=on
