# See docs/devel/tracing.txt for syntax documentation.

# hw/sd/milkymist-memcard.c
milkymist_memcard_memory_read(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
milkymist_memcard_memory_write(uint32_t addr, uint32_t value) "addr 0x%08x value 0x%08x"
